SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( M2860020bspor
 Type ( Engine )
 WagonShape ( Csd_M286bs.s )
 Size ( 3.11m 4.23m 24.49m )
 Mass ( 53.0t )
 WheelRadius ( 0.46m )
 InertiaTensor ( Box (3.11m 4.23m 24.49m) )
Comment (verze ladeni 20-11-2006 - dle norem Ppoollll nastavil Semora)
Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5E6N/m 1E7N/m )
			Damping ( 1E6N/m/s 2E6N/m/s )
			Break ( 1.1E7N 5E7N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5E6N/m 1E7N/m )
			Damping ( 1E6N/m/s 2E6N/m/s )
			Break ( 1.1E7N 5E7N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1E6N/m 5E6N/m )
			Damping ( 1E6N/m/s 1E6N/m/s )
			r0 ( 60cm 30cm )
		)
		Centre ( 0.5m )
		Radius ( 1m )
		Angle ( 0.5deg )
	)
 Adheasion ( 0.2 0.4 2 0 )
 DerailRailHeight ( 4cm )
 DerailRailForce ( 400kN )
 DerailBufferForce ( 300kN )
 NumWheels ( 4 )

 Friction (
  120N/m/s  1  -1mph        0  1
  5.1N/rad/s  1  -1rad/s  0  1
 )

 BrakeEquipmentType ( "Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )

 BrakeSystemType ( "Air_single_pipe" )
 comment ( 0.1 - 0.16 tihy, volim 0.11, takze 0.11*460.000=50.6 )
 MaxBrakeForce ( 58kN )
 
 EmergencyBrakeResMaxPressure( 60 )
 TripleValveRatio( 2.5 )
 MaxReleaseRate( 4.2 )
 MaxApplicationRate( 15 )
 MaxAuxilaryChargingRate( 0.8 )
 EmergencyResCapacity( 2 )
 EmergencyResChargingRate( 0.8 )
 BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )

 IntakePoint ( 0 1.0 FuelDiesel )

      PassengerCapacity ( 80.0 )

 Lights ( 8

		Light ( comment ( 6 zadni cervene leve )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
				)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ccFF0000 )
					Position ( -0.889 1.484 -11.875 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
				)
			)
		Light ( comment( 8 zadni cervene prave )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
				)
			FadeIn ( 0.1 )
			FadeOut	( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( ccff0000 )
					Position ( 0.889 1.484 -11.875 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
				)
			)

		Light ( comment ( 2 predni cervene leve )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
				Service ( 2 )
				)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ccFF0000 )
					Position ( -0.889 1.484 11.875 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
				)
			)
		Light ( comment( 4 Predni cervene prave )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
				Service ( 2 )
				)
			FadeIn ( 0.1 )
			FadeOut	( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( ccff0000 )
					Position ( 0.889 1.484 11.875 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
				)
			)

		comment( Definice svetel pro loko LOOSE CONSIST )

		Light ( comment ( Predni pravy ODSTAVENA NOC )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				Service ( 1 )
				Control ( 0 )
				TimeOfDay ( 2 )
				Penalty ( 1 )
				)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( aaffeba4 )
					Position ( 0.889 1.484 11.875 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					)
				)
			)
		Light ( comment ( Predni levy ODSTAVENA NOC )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				Service ( 1 )
				Control ( 0 )
				TimeOfDay ( 2 )
				Penalty ( 1 )
				)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( aaffeba4 )
					Position ( -0.889 1.484 11.875 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					)
				)
			)
		Light ( comment ( Zadni pravy ODSTAVENA NOC )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				Service ( 1 )
				Control ( 0 )
				TimeOfDay ( 2 )
				)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( aaffeba4 )
					Position ( 0.889 1.484 -11.875 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.4 )
     					)
				)
			)
		Light ( comment ( Zadni levy ODSTAVENA NOC )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				Service ( 1 )
				Control ( 0 )
				TimeOfDay ( 2 )
				)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( aaffeba4 )
					Position ( -0.889 1.484 -11.875 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.4 )
                                        )
                                    )
				)
                            )

)
 Engine ( M2860020bspor
 Wagon ( M2860020bspor )
 Type ( Diesel )
 MaxPower ( 1kW )
 MaxForce ( 1kN )
 MaxContinuousForce ( 1kN )
 MaxVelocity ( 110km/h )
 WheelRadius ( 0.45m )

 NumWheels ( 4 )
 MaxTemperature ( 120 )
 MaxOilPressure ( 90 )

 AirBrakesAirCompressorPowerRating( 0.05 )
 AirBrakesMainMinResAirPressure( 0 )
 AirBrakesMainMaxAirPressure( 112 )
 AirBrakesMainResVolume( 1.5 )
 AirBrakesAirCompressorWattage( 9000 )
 AirBrakesCompressorRestartPressure( 80 )
 AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.34 )
 AirBrakesIsCompressorElectricOrMechanical( 0 )

 EngineBrakesControllerMinPressureReduction( 0 )
 TrainBrakesControllerMinPressureReduction( 0 )
 EngineBrakesControllerHasProportionalBrake( 1 )
 EngineBrakesProportionalBrakeLag( 1 )
 EngineBrakesControllerMaxApplicationRate( 1.9 )
 TrainBrakesControllerMaxApplicationRate( 1.9 )
 EngineBrakesControllerMaxReleaseRate( 1.4 )
 TrainBrakesControllerMaxReleaseRate( 2 )
 EngineBrakesControllerEmergencyApplicationRate( 15 )
 TrainBrakesControllerEmergencyApplicationRate( 15 )
 EngineBrakesControllerMinSystemPressure( 0 )
 TrainBrakesControllerMinSystemPressure( 0 )
 EngineBrakesControllerMaxSystemPressure( 73 )
 TrainBrakesControllerMaxSystemPressure( 73 )
 EngineBrakesControllerEmergencyBrakeTimePenalty( 10 )
 TrainBrakesControllerEmergencyBrakeTimePenalty( 10 )
 EngineBrakesControllerFullServicePressureDrop( 35 )
 TrainBrakesControllerFullServicePressureDrop( 35 )


 BrakesEngineBrakeType ( "Air_single_pipe"  )
 BrakesTrainBrakeType ( "Air_single_pipe" )
 BrakesEngineControllers( "Independent, Train" )

 EngineBrakesControllerDirectControlExponent( 1 )
 
 MaxDieselLevel ( 1600l )
      DieselUsedPerHourAtMaxPower ( 148l )
 DieselUsedPerHourAtIdle ( 7l )

 DieselSmokeEffectInitialMagnitude( 1.5 )
 DieselSmokeEffectMaxMagnitude( 1.9 )
 DieselSmokeEffectInitialSmokeRate( 0.5 )
 DieselSmokeEffectMaxSmokeRate( 2.5 ) 
 
 DieselEngineIdleRPM( 650 )
 DieselEngineMaxRPM( 1400 ) 
 DieselEngineSpeedOfMaxTractiveEffort( 23km/h )        
      DieselEngineMaxRPMChangeRate( 230 )

 DoesHornTriggerBell( 0 )
EngineVariables( 240 )
   
        EngineControllers (           
            Brake_Hand ( 0 1 0.030 0
       NumNotches( 1
                    Notch(0    1 Dummy)
                )
            )
            )

      Sound (  "../../common.snd/vozy/CDvuzOs4nEx.sms" )
     Name ("CSD M286.0020 mimo provoz")
       Description (
	"Motorovy vuz 850 CSD ( ex. M286.0 )\n\n"+
	"Univerzalni motorovy vuz pro \n"+
	"osobni, spesne vlaky i rychliky "+
	"na neelektrifikovanych tratich. "+
	"Prenos vykonu: hydraulicky, pres MMM prevodovku\n\n"+
	"Motor: CKD K12V170DR \n\n"+
	"Vykon: 515kW pri 1400min-1 \n\n"+
	"Max. rychlost: 110km/h\n\n"+
	"Delka pres narazniky: 24790mm\n\n"+
	"Hmotnost: 50-59t\n\n"+
	"Napravy: 4, usporadani B'2'\n\n"+
	"Vyroba: Vagonka Studenka, 1966-67"
     )

)